{"text_format":"1","workbook":"xlsx","n_sheets":23,"sheets":["Home","Bubbler","Shaft Encoder","Radar","Pressure Transducer","Ultrasonic Sensor","Gate Sensor","AWS","Rain Gauge","Rain and Snow Gauge","Snow Depth","INSAT","VSAT","GSM","Datalogger 1","Datalogger 2","Water Quality","ADCP","Power","GW Level with Datalogger","GW Level Non-Vented Cable","GW Level Vented Cable","GW Level No Cable"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Home","index":0,"n_rows":48,"n_cols":30,"rows_kept":48,"cut":false,"hidden":false,"merged":[[3,1,3,7],[3,9,3,15],[13,9,13,15],[3,17,3,23],[13,17,13,23]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat1 Rain Only"]
[null,null,null,"Select State",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RainCheck",true,null,"Uttrakhand or Himachal Pradesh"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GSM / GPRS",1,null,"Other States except Uttrakhand or Himachal"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSAT Radio",null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VSAT"]
[null,null,"Select Telemetry Option",null,null,null,null,null,null,null,"Select Telemetry Option",null,null,null,null,null,null,null,"Select Telemetry Option",null,null,null,null,null,null,null,"Rain Gauges only",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Snow Precipitation Sensor",true]
[null,null,"Select Sensor Type",null,null,null,null,null,null,null,"Solar Radiation Sensor",null,null,null,null,null,null,null,"Sensor Selection",null,null,null,null,null,null,null,"Both of Above"]
[]
[null,null,null,null,null,null,null,null,null,null,"Wind Velocity / Direction",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat 2 WL Only"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WLCheck",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telemetry",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Shaft Encoders",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Radar",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ultrasonic Sensor",true]
[null,null,"Select Telemetry Option",null,null,null,null,null,null,null,"Select Telemetry Option",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bubbler",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Depth Range",null,null,null,null,null,null,"Pressure Transducer",true]
[null,null,"Select Sensor Types",null,null,null,null,null,null,null,"Sensor Type"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat3 AWS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AWSCheck",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telemetry",3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Thermopile Based",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Silicon Photovoltaic Cell"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ultrasonic Sensor",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cup Anemometer and Vane"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat4 GWL",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telemetry",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"With Vent Pipe",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Without Vent Pipe"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat5 WQ",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telemetry",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sonde",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Depth",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Conductivity",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dissolved Oxygen",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turbidity",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pH",true]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cat6 Discharge",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"chk ADCP",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Upto 6 meter",3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Upto 25 meter"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Above 25 meter"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"chk ADVM",true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telemetry",2]

{"sheet":"Bubbler","index":1,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[[17,1,17,2],[6,1,6,2],[2,1,2,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"(*) Sensor Type","Continuous bubbling system and non-submersible transducer"]
[null,"(*) Range","15 PSI"]
[null,"(*) Resolution","3 mm @ 15 PSI  or better"]
[null,"(*) Accuracy","0.02 % FSO"]
[null,"Output Interface","SDI-12 / 4-20 mA / RS485, compatible with Data logger"]
[null,"Power Supply","11 to 15 V DC"]
[null,"Average current Draw","<15mA based on 1 bubble per second"]
[null,"Purge","Manual line purge"]
[null,"Bubble Rate","Programmable 30–120 bubbles per minute"]
[null,"(*) Desiccator","The bubbling mechanism and the non-submersible transducer must be equipped with a desiccating system to keep system from malfunction for a period not less than 6 months."]
[null,"General Features"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]
[null,"(*) Enclosure","NEMA4 or IP64"]

{"sheet":"Shaft Encoder","index":2,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[[20,1,20,2],[2,1,2,2],[6,1,6,2],[13,1,13,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"(*) Sensor Type","Shaft Encoder based rotary position sensor with Digital Display"]
[null,"(*) Range","1-100 meter"]
[null,"(*) Resolution","3 mm or less"]
[null,"(*) Accuracy","0.025 % FSO"]
[null,"Output Interface","SDI-12 / RS 485 / 4-20 mA / compatible with data logger"]
[null,"Power Supply","12 V DC or Switch rated for 12 V DC"]
[null,"General Features"]
[null,"Material","Corrosion Resistance Metal (Stainless steel or Aluminum)"]
[null,"(*) Enclosure","Lockable (key) box provided by the supplier to be mounted in Stilling well or Gauge hut, with IP65 or NEMA 4 protection"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Graduated Tape","The tape should be of high quality to withstand harsh and humid environment, should not get twisted or wrinkeled while operation."]
[null,"Accessaries","Sensor Mounting support, Floats, graduated tapes (metric), wheel, counterweight, and cabling"]

{"sheet":"Radar","index":3,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[13,1,13,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"(*) Sensor Type","Microwave non-contact sensor"]
[null,"(*) Range","30 meter"]
[null,"(*) Resolution","3 mm  or better"]
[null,"(*) Accuracy","0.02 % FSO"]
[null,"Output Interface","SDI-12 / RS 485 / 4-20 mA / compatible with data logger"]
[null,"Power Supply","10-15 V DC"]
[null,"General Features"]
[null,"Material","Corrosion Resistance Metal (Stainless steel / Aluminum or PVC)"]
[null,"Enclosure","The Sensor shall be easy to dismount and replace in the event of malfunction.  "]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]
[null,"(*) Protection","NEMA 4 or IP64"]

{"sheet":"Pressure Transducer","index":4,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[13,1,13,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"(*) Sensor Type","Pressure Sensor"]
[null,"(*) Range","30 meter"]
[null,"(*) Resolution","3 mm  or better"]
[null,"(*) Accuracy","0.02 % FSO"]
[null,"Output Interface","SDI-12 / RS 485 / 4-20 mA / compatible with data logger"]
[null,"Power Supply","10-15 V DC"]
[null,"General Features"]
[null,"Material","Corrosion Resistance Metal (Stainless steel / Aluminum or PVC)"]
[null,"Enclosure","The Sensor shall be easy to dismount and replace in the event of malfunction.  "]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]
[null,"(*) Protection","NEMA 4 or IP64"]

{"sheet":"Ultrasonic Sensor","index":5,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[13,1,13,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"(*) Sensor Type","Ultrasonic non-contact sensor"]
[null,"(*) Range","10 meter"]
[null,"(*) Resolution","3 mm  or better"]
[null,"(*) Accuracy","0.02 % FSO"]
[null,"Output Interface","SDI-12 / RS 485 / 4-20 mA / compatible with data logger"]
[null,"Power Supply","10-15 V DC"]
[null,"General Features"]
[null,"Material","Corrosion Resistance Metal (Stainless steel / Aluminum or PVC)"]
[null,"Enclosure","The Sensor shall be easy to dismount and replace in the event of malfunction.  "]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]
[null,"(*) Protection","NEMA 4 or IP64"]

{"sheet":"Gate Sensor","index":6,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[[20,1,20,2],[2,1,2,2],[6,1,6,2],[11,1,11,2],[19,1,19,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +50 Degree C"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Incremental / Absolute encoder"]
[null,"Range","0-4 meter"]
[null,"Resolution","1 mm or less"]
[null,"Accuracy","0.025 % FSO"]
[null,"General Features"]
[null,"Output Interface","SDI-12 / RS 485 / 4-20 mA / compatible with datalogger"]
[null,"Power Supply","12 V DC or switch compatible with 12 VDC"]
[null,"Material","Corrosion Resistance Metal (Stainless steel or Aluminium)"]
[null,"Enclosure","Outdoor environment with corosion resistant material"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessaries","Sensor Mounting support,  cabling etc"]
[null,"Specific Features"]
[null,"It should accept safety inputs like Gate faulty, Gate in Manual (handle on), Gate tide up etc. and convey it to data logger. "]

{"sheet":"AWS","index":7,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[[12,1,12,2],[2,1,2,2],[6,1,6,2],[23,1,23,2],[35,1,35,2],[18,1,18,2],[29,1,29,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Temperature Sensor"]
[null,"Sensor Type","Resistance type Temperature Sensor"]
[null,"Range","-20 to 60 Degree C"]
[null,"Resolution","± 0.1°C"]
[null,"Accuracy (Intensity)","0.3°C or better"]
[null,"Power Supply","12 V DC or switch rated for 12 VDC"]
[null,"Humidity Sensor"]
[null,"Sensor Type","Capacitive/ Solid State Humidity Sensor"]
[null,"Range","5 to 100 %"]
[null,"Resolution","0.5 Percent"]
[null,"Accuracy","±3% or better"]
[null,"Power Supply","12 V DC or switch rated for 12 VDC"]
[null,"Wind Speed and Direction Sensor",null,null,"Option 1","Option 2"]
[null,"Sensor Type",{"$f":"IF(Home!$AB$24=1,AWS!E20,AWS!F20)","v":"Ultrasonic sensor (No moving Parts)"},null,"Ultrasonic sensor (No moving Parts)","Non-Contact encoders with cup anemometer and wind vane"]
[null,"Range",{"$f":"IF(Home!$AB$24=1,AWS!E21,AWS!F21)","v":"65m/s for speed ;\n0–360 degrees for direction"},null,"65m/s for speed ;\n0–360 degrees for direction","0.3 to 65m/s for speed; \n0–360 degrees for direction"]
[null,"Resolution",{"$f":"IF(Home!$AB$24=1,AWS!E22,AWS!F22)","v":"0.01 m/s for Speed; \n0.1 degree for Direction"},null,"0.01 m/s for Speed; \n0.1 degree for Direction","0.01 m/s for speed; \n0.1 degree for direction"]
[null,"Accuracy",{"$f":"IF(Home!$AB$24=1,AWS!E23,AWS!F23)","v":"0.2 m/s or 3% for wind speed;\n+/- 2 degrees for direction"},null,"0.2 m/s or 3% for wind speed;\n+/- 2 degrees for direction","0. 4 m/s for speed; \n+/- 5 degrees for direction"]
[null,"Pressure Sensor"]
[null,"Sensor Type","Temperature Compensated"]
[null,"Range","800 - 1200 hPa"]
[null,"Resolution"," ± 0.01 hPa"]
[null,"Accuracy"," ± 0.5 hPa"]
[null,"Power Supply","12 V DC or switch rated for 12 VDC"]
[null,"Solar Radiation Sensor",null,null,"Option 1","Option 2"]
[null,"Sensor Type",{"$f":"IF(Home!$AB$22=1,AWS!E31,AWS!F31)","v":"Silicon photovoltaic detector"},null,"ISO Class 1 Pyranometer (CMP 11 or better)","Silicon photovoltaic detector"]
[null,"Spectral Range",{"$f":"IF(Home!$AB$22=1,AWS!E32,AWS!F32)","v":"400-1000 nm"},null,"300-1000 nm","400-1000 nm"]
[null,"Range",{"$f":"IF(Home!$AB$22=1,AWS!E33,AWS!F33)","v":"0-2000 W/Square meter"},null,"0-2000 W/Square meter","0-2000 W/Square meter"]
[null,"Resolution",{"$f":"IF(Home!$AB$22=1,AWS!E34,AWS!F34)","v":"1 W/Square meter"},null,"1 W/Square meter","1 W/Square meter"]
[null,"Accuracy (Including Temperature Compensation)",{"$f":"IF(Home!$AB$22=1,AWS!E35,AWS!F35)","v":0.05},null,0.03,0.05]
[null,"General Features"]
[null,"Material","Corrosion Resistance Metal (Stainless steel/  Aluminum or PVC)"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]
[null,"Output Interface","SDI 12/RS 485/ 4-20 mA/ Compatible with Data logger"]

{"sheet":"Rain Gauge","index":8,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[[19,1,19,2],[2,1,2,2],[6,1,6,2],[11,1,11,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -5 to +50 Degree C"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 2000 meter"]
[null,"Sensor",null,null,"Option 1","Option 2","Option 3"]
[null,"Sensor Type","Tipping Bucket reed switch"]
[null,"Range","0-250 mm/h"]
[null,"Resolution","0.5 mm",null,"0.2 mm","0.5 mm","1 mm"]
[null,"Accuracy (Intensity)","2 % or better"]
[null,"General Features"]
[null,"Output Interface","SDI12/ RS 485 / Compatible with Data logger"]
[null,"Material","Corrosion Resistance Metal (Stainless steel/ Aluminum or PVC)"]
[null,"Enclosure","Ability to service tipping buckets without involving the re-leveling of the gauge."]
[null,"Protection","NEMA 4 or IP65"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessaries","Sensor Mounting support, cables and other accessories as required"]
[null,"Specific Features"]
[null,"Collecting Funnel Diameter ","200 mm or 8 Inch or equivalent"]
[null,"Insect Screen","Insect covers on all openings should be provided"]

{"sheet":"Rain and Snow Gauge","index":9,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[[19,1,19,2],[2,1,2,2],[6,1,6,2],[11,1,11,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -40 to +50 Degree C"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Storage Gauge with Anti-freeze system without heating"]
[null,"Capacity","1000 mm minimum"]
[null,"Resolution","0.5 mm  or better"]
[null,"Accuracy (Intensity)","2 % or better, ±2 mm"]
[null,"General Features"]
[null,"Output Interface","SDI12/ RS 485 / Compatible with Data logger"]
[null,"Power Supply","12 V DC or switch rated for 12 VDC"]
[null,"Material","Corrosion Resistance Metal (Stainless steel or Aluminum)"]
[null,"Enclosure","NEMA 4"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessaries","Sensor Mounting support, cables and other accessories as required"]

{"sheet":"Snow Depth","index":10,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[[19,1,19,2],[2,1,2,2],[6,1,6,2],[11,1,11,2]]}
[]
[null,"Feature","Units"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Ultrasonic sensor"]
[null,"Range","0-10 meter"]
[null,"Resolution","1 mm  or better"]
[null,"Accuracy","0.25 % of measuring distance"]
[null,"General Features"]
[null,"Output Interface","SDI12/ RS 485 / Compatible with Data logger"]
[null,"Power Supply","9-18 V DC"]
[null,"Material","Corrosion Resistance Metal (Stainless steel/  Aluminum or PVC)"]
[null,"Enclosure","NEMA 4"]
[null,"Tools","Complete tool kit for operation and routine maintenance"]
[null,"Manuals","Full Documentation and maintenance manual in English"]
[null,"Accessories","Sensor Mounting support, cables and other accessories as required"]

{"sheet":"INSAT","index":11,"n_rows":23,"n_cols":4,"rows_kept":23,"cut":false,"hidden":false,"merged":[[18,1,18,2],[10,1,10,2]]}
[]
[null,"Feature","Value"]
[null,"Operating Temperature","From -20 to +60","From -20 to +60"]
[null,"Environment Relative Humidity","0 to 100 %"]
[null,"Career Frequency","402 - 403 MHz"]
[null,"Output Power","3-10 W, user settable"]
[null,"Data Bit Rate","4.8 kbps"]
[null,"Antenna cable ","LMR 400 grade or better"]
[null,"Performance","Data Reception availability of 99% or better"]
[null,"Form factor","The Transmitter should either be integral part of data logger specified above, or it should be supplied as independent unit compatible with supplied data logger"]
[null,"Yagi Antenna"]
[null,"Polarization","LHCP or RHCP, switchable in field"]
[null,"Gain","Minimum 11 dbi or better"]
[null,"Center Frequency","402-403 MHz"]
[null,"Mounting","Proper mounting and Pointing arrangement for 360 degree azimuth and elevation adjustment"]
[null,"Operating Wind speed","250 kmph"]
[null,"Wind Survival","300 kmph"]
[null,"Material","Rust-proof and Oxidation-proof"]
[null,"Specific Features"]
[null,"Satellite System","INSAT Radio System to be Used on the INSAT Satellite operated by ISRO"]
[null,"Certification","Certificate of acceptance required by ISRO and/or IMD as part of the bid package"]
[null,"Demonstration in India","Demonstrated use of the satellite radio with at least 200 radios in current operation in India using INSAT"]
[null,"Accessories","All associated equipment, including GPS, GPS Antenna, INSAT Antenna, all cables and mounting hardware"]

{"sheet":"VSAT","index":12,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[]
[null,"Feature","Value"]
[null,"Operating Temperature","From -20 to +60"]
[null,"Antenna cable ","LMR 400 grade or better"]
[null,"Performance","Data Reception availability of 99% or better"]
[null,"Specific Features"]
[null,"Communication Direction","VSAT Radio system to allow two-way communication system between Data Center and remote station"]
[null,"Single Hop","VSAT communication will be direct link, and use the internet or any surface based topology for data communication (i.e. leased lines)"]
[null,"Bandwidth Sharing","VSAT bandwidth will be able to be shared among all stations"]
[null,"Alarm Conditions","VSAT remote stations shall be able to transmit based on alarm conditions at the remote site such as critical water level or exceptional precipitation events"]
[null,"Accessories","All associated equipment, including Antenna all cables and mounting hardware"]

{"sheet":"GSM","index":13,"n_rows":12,"n_cols":3,"rows_kept":12,"cut":false,"hidden":false,"merged":[[5,1,5,2]]}
[]
[null,"Feature","Value"]
[null,"Operating Temperature","From -20 to +60"]
[null,"Performance","Data Reception availability of 95% or better"]
[null,"Form factor","The Transmitter should either be integral part of data logger specified above, or it should be supplied as independent unit compatible with supplied data logger"]
[null,"Specific Features"]
[null,"Communication Direction","Utilize GPRS network for two-way TCP/IP (INTERNET) connection"]
[null,"VPN protocol","Radio to utilize VPN protocol"]
[null,"Transmission trigger","Data collection to be triggered by interrogation from Data Center, or by event based transmission triggered by remote site"]
[null,"Power Saving","Ability to disable interrogation system in order to save power at remote site"]
[null,"Communication Protocol","Data transmission to execute HTTP Post or FTPS to transmit data to the Data Center"]
[null,"Accessories","All associated equipment, including Antenna all cables and mounting hardware"]

{"sheet":"Datalogger 1","index":14,"n_rows":37,"n_cols":3,"rows_kept":37,"cut":false,"hidden":false,"merged":[[2,1,2,2],[17,1,17,2],[21,1,21,2],[6,1,6,2],[11,1,11,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +50 Degree C"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor Interface"]
[null,"Analogue Inputs","8 Analogue Input Channels"]
[null,"SDI Port","One SDI-12 Interface port"]
[null,"Digital Inputs","6 Digital Channels, bidirectional"]
[null,"Pulse Input","2 Input for Rain Gauge impulse"]
[null,"Input - Output Interfaces"]
[null,"Data Transfer","USB stick option for Data transfer"]
[null,"Port for Configuration","One Serial Port (RS232) for communication with Laptop or programming"]
[null,"Serial / RS 485","One for the INSAT radio"]
[null,"RS232","One for the addition of GSM radio "]
[null,"LAN Port","RJ 45 port for LAN / VSAT"]
[null,"Computer Software"]
[null,"Operating System","Windows software for system configuration / communication"]
[null,"Version","English language version"]
[null,"Licenses","All required licenses included"]
[null,"General Features"]
[null,"Flash memory","Non-volatile Flash memory that can one store year of data and expandable to a minimum of 1GB."]
[null,"Resolution","A/D resolution ≥16 bit"]
[null,"Recording Interval","Individual recording intervals for each sensor/parameter"]
[null,"Firmware Operating System","Multi-tasking operating system - must log data and transmit at same time"]
[null,"Display","Digital Display for viewing current data and setting values"]
[null,"Power Supply","Power supply 12V DC, low current drain (quiescent ≤10.0mA)"]
[null,"Battery Voltage","Monitoring of battery voltage level"]
[null,"Internal battery","Internal battery backup for clock"]
[null,"User Permissions","Different user levels, system of user rights / passwords, access restricted to authorized personnel"]
[null,"Internal clock","Internal clock with drift less than 2 seconds per day or using GPS"]
[null,"System integrity","System integrity check procedures"]
[null,"Enclosure","for wall-mounting in a shelter / enclosure with IP65 (NEMA 4) protection or better"]
[null,"Accessories","Serial cable + adaptor (if required) for notebook connection. All accessories (fixing units, etc.) as required"]
[null,"Tools","complete tool kit for installation and routine maintenance giving full detail( number of pieces and type) "]
[null,"Manuals","full documentation and maintenance instructions in English (1 copy per station)."]

{"sheet":"Datalogger 2","index":15,"n_rows":35,"n_cols":3,"rows_kept":35,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[11,1,11,2],[15,1,15,2],[19,1,19,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +50 Degree C"]
[null,"Humidity","5 to 100 %"]
[null,"Altitude","0 to 5000 meter"]
[null,"Sensor Interface"]
[null,"Analogue Inputs","8 Analogue Input Channels"]
[null,"SDI Port","One SDI-12 Interface port"]
[null,"Digital Inputs","6 Digital Channels, bidirectional"]
[null,"Pulse Input","2 Input for Rain Gauge impulse"]
[null,"Input - Output Interfaces"]
[null,"Data Transfer","USB stick option for Data transfer"]
[null,"Port for Configuration","One Serial Port (RS232) for communication with Laptop or programming"]
[null,"Port for Telemetry","Port for Communication with Telemetry Device (GSM/VSAT/INSAT) specified below"]
[null,"Computer Software"]
[null,"Operating System","Windows software for system configuration / communication"]
[null,"Version","English language version"]
[null,"Licenses","All required licenses included"]
[null,"General Features"]
[null,"Flash memory","Non-volatile Flash memory that can one store year of data and expandable to a minimum of 1GB."]
[null,"Resolution","A/D resolution ≥16 bit"]
[null,"Recording Interval","Individual recording intervals for each sensor/parameter"]
[null,"Firmware Operating System","Multi-tasking operating system - must log data and transmit at same time"]
[null,"Display","Digital Display for viewing current data and setting values"]
[null,"Power Supply","Power supply 12V DC, low current drain (quiescent ≤10.0mA)"]
[null,"Battery Voltage","Monitoring of battery voltage level"]
[null,"Internal battery","Internal battery backup for clock"]
[null,"User Permissions","Different user levels, system of user rights / passwords, access restricted to authorized personnel"]
[null,"Internal clock","Internal clock with drift less than 2 seconds per day or using GPS"]
[null,"System integrity","System integrity check procedures"]
[null,"Enclosure","for wall-mounting in a shelter / enclosure with IP65 (NEMA 4) protection or better"]
[null,"Accessories","Serial cable + adaptor (if required) for notebook connection. All accessories (fixing units, etc.) as required"]
[null,"Tools","complete tool kit for installation and routine maintenance giving full detail( number of pieces and type) "]
[null,"Manuals","full documentation and maintenance instructions in English (1 copy per station)."]

{"sheet":"Water Quality","index":16,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[[2,4,2,5],[6,4,6,5],[10,4,10,5],[14,4,14,5],[32,4,32,5],[18,4,18,5],[32,1,32,2],[36,1,36,2],[23,4,23,5],[27,4,27,5],[36,4,36,5],[2,1,2,2],[6,1,6,2],[18,1,18,2],[27,1,27,2],[10,1,10,2],[23,1,23,2],[14,1,14,2]]}
[]
[null,"Feature","Value",null,"Feature","Value"]
[null,"Site Conditions",null,null,"Site Conditions"]
[null,"Ambient Temperature","-5 to 45 Degree C",null,"Ambient Temperature","-5 to 45 Degree C"]
[null,"Humidity","5-100 %",null,"Humidity","5-100 %"]
[null,"Altitude","0-5000 meter",null,"Altitude","0-5000 meter"]
[null,"Multi parameter Sonde",null,null,"Multi parameter Sonde"]
[null,"Ports","6 or more",null,"Ports","6 or more"]
[null,"Response Time","<90 s",null,"Response Time","<90 s"]
[null,"Output","SDI-12, RS-232",null,"Output","SDI-12, RS-232"]
[null,"Depth",null,null,"Depth"]
[null,"Accuracy","0.003 m",null,"Accuracy","0.003 m"]
[null,"Resolution","0.001 m",null,"Resolution","0.001 m"]
[null,"Range","0 to 60m",null,"Range","0 to 60m"]
[null,"Conductivity",null,null,"Conductivity"]
[null,"Accuracy"," +/- 3% FS or 5μS/cm",null,"Accuracy"," +/- 3% FS or 5μS/cm"]
[null,"Resolution",null,null,"Resolution"]
[null,"Range"," 0 - 100 μS/cm",null,"Range"," 0 - 100 μS/cm"]
[null,"Dissolved oxygen (optical)",null,null,"Dissolved oxygen (optical)"]
[null,"Accuracy"," +/- 5% reading \nor +/- 0.2 mg/L",null,"Accuracy"," +/- 5% reading \nor +/- 0.2 mg/L"]
[null,"Resolution","0.01 mg/L",null,"Resolution","0.01 mg/L"]
[null,"Range","0 to 50 mg/L",null,"Range","0 to 50 mg/L"]
[null,"Sensor Cleaning","Automated sensor cleaning mechanism",null,"Sensor Cleaning","Automated sensor cleaning mechanism"]
[null,"Temperature",null,null,"Temperature"]
[null,"Accuracy"," +/- 0.2oC",null,"Accuracy"," +/- 0.2oC"]
[null,"Resolution","0.2oC",null,"Resolution","0.2oC"]
[null,"Range"," -5 to 45o C",null,"Range"," -5 to 45o C"]
[null,"Turbidity",null,null,"Turbidity"]
[null,"Accuracy"," +/- 5% reading or 2 NTU",null,"Accuracy"," +/- 5% reading or 2 NTU"]
[null,"Resolution","1 NTU",null,"Resolution","1 NTU"]
[null,"Range","0 to 1000 NTU",null,"Range","0 to 1000 NTU"]
[null,"Sensor Cleaning","Automated sensor cleaning mechanism",null,"Sensor Cleaning","Automated sensor cleaning mechanism"]
[null,"pH",null,null,"pH"]
[null,"Accuracy"," +/- 0.2 pH units;  +/- 1.0 mV",null,"Accuracy"," +/- 0.2 pH units;  +/- 1.0 mV"]
[null,"Resolution","0.01 pH unit; 0.1 mV",null,"Resolution","0.01 pH unit; 0.1 mV"]
[null,"Range","2 - 12 pH units (minimum) ; 0-14 pH units (Preferred)",null,"Range","2 - 12 pH units (minimum) ; 0-14 pH units (Preferred)"]
[null,"General Features",null,null,"General Features"]
[null,"Tools","Complete tool kit for installation and routine maintenance",null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English",null,"Manuals","Full documentation and maintenance instructions in English"]

{"sheet":"ADCP","index":17,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[[17,1,17,2],[22,1,22,2],[2,1,2,2],[6,1,6,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","-5 to 45 Degree C"]
[null,"Humidity","5-100 %"]
[null,"Altitude","0-5000 meter"]
[null,"Sensor"]
[null,"ADCP Type","Broadband ADCP for measurement of discharge in open channel environment",null,"Option 1","Option 2","Option 3"]
[null,"Profiling Range",{"$f":"IF(Home!AB44=1,ADCP!E9,IF(Home!AB44=2,ADCP!F9,ADCP!G9))","v":"0.5–60m"},null,"0.3–10m","0.4–25m","0.5–60m"]
[null,"Profiling Velocity","+/-20 m/s"]
[null,"Velocity Accuracy","0.25% of measured velocity"]
[null,"Velocity Resolution","0.001m/s"]
[null,"Depth Range","0.3-80 m"]
[null,"Depth Accuracy","1%."]
[null,"Depth Resolution","0.001 m"]
[null,"Positioning","Optional capability to acquire position by bottom tracking or integrated GPS."]
[null,"Computations","All performed internally or on Windows-based software (supplied)"]
[null,"Accessories"]
[null,"Platform","Floating platform for tethered ADCP deployment"]
[null,"Positioning","GPS for positioning"]
[null,"Tethers","All necessary tethers and taglines "]
[null,"Software","Windows-based software for display of velocity, discharge, depth, and width information in real-time."]
[null,"General Features"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]

{"sheet":"Power","index":18,"n_rows":12,"n_cols":3,"rows_kept":12,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[11,1,11,2],[10,1,10,2]]}
[]
[null,"Feature","Units"]
[null,"Battery"]
[null,"Voltage","From -20 to +60"]
[null,"Type","Sealed Maintenance free"]
[null,"Capacity","Based on site conditions and Telemetry method, to provide 21 days of backup"]
[null,"Solar Panels"]
[null,"Size","Based on Site conditions and Telemetry method used for 21 days of backup"]
[null,"Mounts","The mounts should be sturdy in design; the solar panel should not move or rotate with wind. It should have provision to adjust direction and elevation during installation for optimal solar power generation"]
[null,"Charger","Smart solar charger with protection"]
[null,"General"]
[null,"The supplier should determine optimal size of solar panels and batteries, such that system should be operational for at least 21 days in the absence of charging"]

{"sheet":"GW Level with Datalogger","index":19,"n_rows":34,"n_cols":3,"rows_kept":34,"cut":false,"hidden":false,"merged":[[30,1,30,2],[18,1,18,2],[2,1,2,2],[6,1,6,2],[14,1,14,2],[26,1,26,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature","From -20 to +60"]
[null,"Humidity","5-100 %"]
[null,"Altitude","0-5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Submersible pressure transducer with atmospheric pressure and temperature compensation"]
[null,"Range","30 psi"]
[null,"Accuracy","0.1% FSO"]
[null,"Resolution","3 mm"]
[null,"Input Power","10-16 VDC"]
[null,"Non-Vented Cable","Includes barometric sensor for post-processing"]
[null,"Output","SDI-12, RS-485"]
[null,"Datalogger"]
[null,"Internal Memory","32 mb"]
[null,"Battery Voltage Monitoring","Monitoring and transmission of Battery Voltage level"]
[null,"Datalogger Location","If Data logger and transmitter are integral parts of sensor, it should be located on top (near ground surface) instead of bottom"]
[null,"GSM / GPRS Transmitter"]
[null,"Performance","Data Reception availability of 95% or better"]
[null,"Communication Direction","Utilize GPRS network for two-way TCP/IP (INTERNET) connection"]
[null,"VPN protocol","Radio to utilize VPN protocol"]
[null,"Transmission trigger","Data collection to be triggered by interrogation from Data Center, or by event based transmission triggered by remote site"]
[null,"Power Saving","Ability to disable interrogation system in order to save power at remote site"]
[null,"Communication Protocol","Data transmission to execute HTTP Post or FTPS to transmit data to the Data Center"]
[null,"Accessories","All associated equipment, including Antenna all cables and mounting hardware"]
[null,"Software"]
[null,"Operating System","Windows software for system configuration,  transfer and analysis of data to computer"]
[null,"Version","English language version"]
[null,"License","All required licenses included"]
[null,"General Features"]
[null,"Battery","The battery should be easy to replace, and easily available in the market"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]

{"sheet":"GW Level Non-Vented Cable","index":20,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[[2,1,2,2],[6,1,6,2],[14,1,14,2],[18,1,18,2]]}
[]
[null,"Feature","Units"]
[null,"Site Conditions"]
[null,"Ambient Temperature"," -10 to +50 Degree C"]
[null,"Humidity","5-100 %"]
[null,"Altitude","0-5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Submersible pressure transducer with atmospheric pressure and temperature compensation"]
[null,"Range","30 psi"]
[null,"Accuracy","0.1% FSO"]
[null,"Resolution","3 mm"]
[null,"Input Power","10-16 VDC"]
[null,"Non-vented cable","Includes barometric sensor for post-processing"]
[null,"Output","SDI-12, RS-485"]
[null,"Software"]
[null,"Operating System","Windows software for system configuration,  transfer and analysis of data to computer"]
[null,"Version","English language version"]
[null,"Licenses","All required licenses included"]
[null,"General Features"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]

{"sheet":"GW Level Vented Cable","index":21,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[[18,1,18,2],[2,1,2,2],[6,1,6,2],[14,1,14,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature"," -10 to +50 Degree C"]
[null,"Humidity","5-100 &"]
[null,"Altitude","0-5000 meter"]
[null,"Sensor"]
[null,"Sensor Type","Submersible pressure transducer with atmospheric pressure and temperature compensation"]
[null,"Range","30 psi"]
[null,"Accuracy","0.1% FSO"]
[null,"Resolution","3 mm"]
[null,"Input Power","10-16 VDC"]
[null,"Vented Cable","Includes mechanism for desiccating vent tube"]
[null,"Output","SDI-12, RS-485"]
[null,"Software"]
[null,"Operating System","Windows software for system configuration,  transfer and analysis of data to computer"]
[null,"Version","English language version"]
[null,"Licenses","All required licenses included"]
[null,"General Features"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]

{"sheet":"GW Level No Cable","index":22,"n_rows":25,"n_cols":3,"rows_kept":25,"cut":false,"hidden":false,"merged":[[17,1,17,2],[21,1,21,2],[2,1,2,2],[6,1,6,2],[13,1,13,2]]}
[]
[null,"Feature","Value"]
[null,"Site Conditions"]
[null,"Ambient Temperature"," -10 to +50 degree C"]
[null,"Humidity","5-100 %"]
[null,"Altitude","0-5000 meter'"]
[null,"Sensor"]
[null,"Sensor Type","Submersible pressure transducer with atmospheric pressure and temperature compensation"]
[null,"Range","30 psi"]
[null,"Accuracy","0.1% FSO"]
[null,"Resolution","3 mm"]
[null,"Input Power","10-16 VDC"]
[null,"No Communication Cable","Internal memory and power supply for at least 1-year operation at one reading per day. Includes barometric sensor for post-processing."]
[null,"Datalogger"]
[null,"Internal Memory","32 mb"]
[null,"Battery Voltage","Monitoring and transmission of Battery Voltage level"]
[null,"Location of Data logger","If Data logger and transmitter are integral parts of sensor, it should be located on top (near ground surface) instead of bottom"]
[null,"Software"]
[null,"Operating System","Windows software for system configuration,  transfer and analysis of data to computer"]
[null,"Version","English language version"]
[null,"Licences","All required licenses included"]
[null,"General Features"]
[null,"Battery","The battery should be easy to replace, and easily available in the market"]
[null,"Tools","Complete tool kit for installation and routine maintenance"]
[null,"Manuals","Full documentation and maintenance instructions in English"]